Tecella VI for Triton + --  Release 1 -- August 11th, 2010

Release 1 notes:

For the Stimulus, please note:
--Stimulus must be at least 2 segments
--Maximum segment length currently is 5 segments
--Only flat segments may be programmed in this release
--Amplitude is in mV when in Vclamp mode and pA when in Iclamp mode

Make sure you adjust the "Chart History Length" when changing the length of the vcmd segments or adding length 
(The chart length cannot be dynamically changed during runtime and I have not figured out a workaround for this)
For example, when doing a total segment length of 300ms, at 20kHz sampling, 6000 samples worth of data has to be shown.
You will have to enter 6000 into Chart History Length. To change this value, right click on the graph and choose
Chart History Length from the dropdown menu. Enter the desired value here.

To select multiple channels when compensating or to view multiple channels, use SHIFT or CTRL keys

--------------------------------------------------------------------------------------------------

The following features are not fully functional and will be functional in future releases:
1. ZAP
2. Stimulus from file
3. System monitor and statistics
4. Callibrate Offset and Callibrate Scale
5. Triggers
6. TLC data format
7. Continuous Acquire

--------------------------------------------------------------------------------------------------

The Following are known issues:
1. Graph recall in Icmd mode views old Vcmd
2. Prepulse present unless auto JP is run
3. Vclamp mode broken on startup when aborted in Icmd mode
